System Settings enter IP of the VAX server ( Default would have been the PC Name )



Edit Panel…set connection mode Static ( panel should be set this way) and IP etc of the Panel



Finally the Panel configuration below should be set as noted.



Results

